{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabella1","Tabella2","Tabella3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabella1","index":0,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[[1,0,1,3],[3,0,3,3],[12,0,12,3],[8,0,8,3],[3,6,3,9],[2,0,2,3],[10,0,10,3]],"flags":["formulas_cached_only"]}
[]
["COMUNE DI OSIO SOTTO (BG)"]
["OFFERTA DELLA DITTA G.R.S. COSTRUZIONI DI OSIO SOTTO ALLEGATA ALLA DET. N° 1164 del 11.12.2017"]
["LAVORI DI FORMAZIONE PAVIMENTO IN CALCESTRUZZO  PRESSO ORTI COMUNALI   "]
["Denominazione commerciale","Quantità","Prezzo ","Totale"]
[" LAVORI DI SCARIFICA CON MINIESACVATORE, SPESSORE CM. 5 E FORMAZIONE DI PIANO DI POSA : SUPERFICIE D'INTERVENTO CIRCA 25 MQ","a corpo","   €. 250,00 "," €. 250,00  "]
["FORMAZIONE DI MASSETTO IN CALCESTRUZZO RCK 30-S4, SPESSORE CM 12/15 CIRCA, TIRATO IN PIANO SOTTO STADIA E FRATAZZATO FINE, COMPRESA FORNITURA E POSA DI RETE ELTTROSALDATA, DOPPIO FOGLIO MAGLIA 20X20 DIAM 6 MM : SUPERFICIE CIRCA 25 MQ ;","a corpo",1000,1000]
[]
["IMPORTO COMPLESSIVO NETTO A BASE D'ASTA PARI AD EURO 1.250,00.="]
[]
["Ribasso offerto dalla Ditta pari al 4% per un importo di affido pari ad Euro 1.200,00.="]
[]
["IL RESPONSABILE DEL PROCEDIMENTO -  F.to  ARCH. DELLA PUPPA MANLIO"]

{"sheet":"Tabella2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabella3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}