{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabella1","Tabella2","Tabella3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabella1","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[[1,0,1,3],[2,0,2,3],[13,0,13,3],[11,0,11,3],[2,6,2,9],[3,0,3,3],[9,0,9,3]],"flags":["formulas_cached_only"]}
[]
["COMUNE DI OSIO SOTTO (BG)"]
[" SOSTITUZIONE VETRO ANTA ASCENSORE SOTTOPASSO "]
["OFFERTA DITTA KONE SPA DI PERO (MI) ALLEGATA ALLA DETERMINA N° 413 DEL 08.05.2018 "]
[]
["Denominazione commerciale","Quantità","Prezzo ","Totale"]
["Fornitura e posa in opera di nuova anta  porta di cabina - piano I° divelta da urto, previo smontaggio della porta attuale per consentire la sostituzione della mezza anta. L'anta è di dimensioni 650 mm di larghezza x 2000 mm di altezza : caratteristiche vetro porta : 5+5+4  0,78 mm - cornice in acciaio inox satinato - Prove e regolazioni funzionali;","n° 1","   €.  2.757,00 "," €.          2.757,00  "]
["TOTALE",null,null,2757]
[]
["IMPORTO COMPLESSIVO NETTO A BASE D'ASTA PARI AD EURO 2.757,00.="]
[]
["Ribasso offerto dalla Ditta pari all'1% sul suddetto importo a base d'asta per un importo di affido pari ad Euro 2.729,43.= + Iva 22%."]
[]
["IL RESPONSABILE DEL PROCEDIMWENTO -  F.to  ARCH. DELLAPUPPA MANLIO"]

{"sheet":"Tabella2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabella3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}